**RECOMMENDED WPCA GUIDELINES FOR GRINDER PUMP SEASONAL SHUTDOWNS:**

**Updated: Sept 2021**

**After six years of monitoring grinder pump winterization , the WPCA now recommends the following :**

**Leave the power on to the grinder pump. Leave the switch in the grinder pump electrical box in the auto position (which is the everyday operating position.)**

**Do not empty the grinder pump. We have found that the keeping the pump under water yields the best results during the early spring pre-season start up.**

Adding Propylene Glycol antifreeze is optional